Rev. 01-29-2025
SECTION 1.10 ENVIRONMENTAL COMPLIANCE 

In Article 1.10.03-Water Pollution Control:
REQUIRED BEST MANAGEMENT PRACTICES

Add the following after Required Best Management Practice Number 13:

  14.	  The Contractor is hereby notified that the location of [Project No.] occurs within a public watershed, aquifer protection area (APA) or sole source aquifer (SSA).  When working in these sensitive resource areas, special requirements must be followed for cleaning machinery, using State property for staging areas, or storing of materials, and servicing/fueling equipment.

All Contractors and their employees must be informed of the sensitive resource area prior to mobilizing on-Site.

No pollutants, as defined in Connecticut General Statue (CGS) Sec. 22a-448 or the Clean Water Act Section 502: General Definitions (6), having adverse effects may be discharged within the public watershed, APA or SSA.

Reporting Requirements

Per CGS Sec. 22a-450-4: Reporting Requirements, any spills or releases of pollutants as defined that cannot be completely cleaned within two hours (regardless of volume) must be reported to Connecticut Department of Energy and Environmental Protection (CTDEEP) within one hour of the discovery by the Contractor.

An unknown material discovery may qualify as a spill or release under the reporting requirements. It is the Contractor’s responsibility to review and understand the nuances of the reporting thresholds requirements of CGS 22a-450-4.

All reportable spills or releases as defined are to be reported by the Contractor to the CTDEEP Emergency Response and Spill Prevention Division (ERSPD) at (860) 424-3338 or toll free at 1-866-337-7745 (1-866-DEPSPIL) and [Water Company] at [XXX-XXX-XXXX], no exceptions. 

When working within the Pootatuck SSA in Newtown, which encompasses areas in Monroe and Easton or within the Pawcatuck SSA in North Stonington, which encompasses areas in Sterling, Stonington and Voluntown, Kira Jacobs from the Environmental Protection Agency (EPA) Region 1 Office must be contacted at (617) 918 -1817. 

In all instances, if a fire or explosion danger exists, the Contractor shall immediately stop all hot work, evacuate the area, call 911, and proceed with other required actions.  Calling 911 does not eliminate the need to contact the Project Engineer and CTDEEP.


Required Best Management Practice

A. All Contractors must adhere to specialized cleanup procedures while working within the public watershed, APA or SSA.
i. The cleaning of all machinery is not to be performed within fifty (50) feet of any wetland or water body within the sensitive resource area.

ii. For cleanup associated with pavers, material transfer vehicles (MTV) and concrete mixers, the Contractor must move the equipment off-line and discharge into a self-contained system.  The self-contained system must be in an acceptable condition and maintained to the satisfaction of the Engineer, as to prevent liquids and solids from permeating through to the ground beneath or adjacent surface areas.  The cleanup area must have oil absorbent pads placed within the self-contained system.  The equipment must be cleaned over the absorbent pads in a manner that will allow the pads to collect any liquids that are used for cleanup.

iii. For cleanup associated with dump trucks, a liquid tight five-gallon pail must be placed at each corner of the dump body below the lower hinges to capture any materials generated during the cleanup.

B. All materials generated during the cleanup procedures must be removed off-Site at the end of each day and disposed of in a manner consistent with all applicable laws and regulations.  These materials shall not be reused within the Project limits or disposed of on State property.  

C. Servicing and fueling of equipment must be conducted outside of a public watershed, APA, or SSA.  If the Contractor cannot conduct work outside of these sensitive resource areas, they must coordinate with the Engineer and comply with the following:

i. Provide a plan sheet identifying the location of the fuel and/or hazardous materials in the Spill Prevention and Remediation Plan for the Engineers review and acceptance.  Fuel and/or hazardous materials must be enclosed within spill proof container throughout the Project duration.

ii. Spill containment systems used during fueling operations shall be manufactured by Sentry Lite Berms, Collapse-a-tainer, or approved equal accepted by the Engineer.  The spill containment system must have a minimum capacity of 
80-gallons and shall be made of plastic or vinyl that is impermeable for all fuel types.

iii. Fuel spill remediation kits must be stored on-Site and identified in the Spill Prevention and Remediation Plan for the Engineers review and acceptance.

D. When working within a public watershed, APA, and/or SSA, the Contractor must submit to the Engineer the desired location of trailer(s), construction staging/laydown areas, containment systems, and sedimentation control systems to the Engineer for review and acceptance prior to the start of construction.

E. Millings may be re-used as asphalt material within the roadway.  Disposal of excess millings must be off-Site in a manner consistent with all applicable laws and regulations.  At no time can millings be placed, dumped, or buried outside of the roadway limits or within State property.

  Attached herein is a copy of the sensitive resource areas map identifying the public watershed, APA or SSA locations within the Project limits.  The resource areas map shall be posted in the Contractor’s and CTDOT inspector’s field offices.
GENERAL
