Metered Service Requirements for Traffic Control Devices in Eversource Territory – 4/4/2025

Traffic control devices with the potential for variable energy consumption (traffic control signals, RRFBs, etc.) shall include metered service.

Items to include:
· 1008129 – 3'' Polyvinyl Chloride Conduit in Trench
· 1008217 – 3" Rigid Metal Conduit Under Roadway
· 1017032A – Service (Metered)

Note: Service cable and riser will be furnished and installed by Eversource. Coordination by the contractor will be covered under item #1017032A – Service (Metered). Service cable from meter socket to main circuit breaker at the traffic cabinet will be paid by the Service (Metered) item along with any grounding and bonding requirements by Eversource.

Special provisions to include:
· NTC – Eversource Metered Service
· 1017032A – Service (Metered)

Traffic Signal Plan:
· Include the following Construction Notes:
· INSTALL A 3” RMC SWEEP AT THE SERVICE POLE AND ATTACH TO THE SERVICE CONDUIT WITH A PVC FEMALE ADAPTER. TO BE PAID FOR UNDER ITEM NO. 1017032A – SERVICE (METERED). BOND AND GROUND RMC SWEEP PER EVERSOURCE REQUIREMENTS. EVERSOURCE TO FURNISH AND INSTALL THE SERVICE RISER AND LINE-SIDE CONDUCTORS.
· SERVICE CONDUIT INSTALLED UNDER THE ROADWAY SHALL BE 3” RMC. A PVC FEMALE ADAPTER SHALL BE USED TO CONNECT TO THE 3” PVC IN TRENCH.





	
